Sec. 7-1809. Field Testing.
Only when inspection indicates that the construction is not in accordance with the approved design, field testing may be required. Interior noise measurements shall be taken under conditions of typical maximum exterior noise levels within legal limits.  A test report showing compliance or noncompliance with prescribed interior allowable levels shall be submitted to the Building Official.